{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":116},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":124,"n_cols":8,"rows_kept":124,"merged":[[0,1,0,2],[0,3,0,4],[0,5,0,7],[1,0,1,7],[2,0,2,7],[4,0,6,0],[4,1,6,1],[4,4,6,4],[4,5,6,5],[4,6,6,6],[4,7,6,7],[7,0,9,0],[7,1,9,1],[7,4,9,4],[7,5,9,5],[7,6,9,6],[7,7,9,7],[10,0,12,0],[10,1,12,1],[10,4,12,4],[10,5,12,5],[10,6,12,6],[10,7,12,7],[13,0,15,0],[13,1,15,1],[13,4,15,4],[13,5,15,5],[13,6,15,6],[13,7,15,7],[16,0,18,0],[16,1,18,1],[16,4,18,4],[16,5,18,5],[16,6,18,6],[16,7,18,7],[19,0,21,0],[19,1,21,1],[19,4,21,4],[19,5,21,5],[19,6,21,6],[19,7,21,7],[22,0,24,0],[22,1,24,1],[22,4,24,4],[22,5,24,5],[22,6,24,6],[22,7,24,7],[25,0,26,0],[25,1,26,1],[25,4,26,4],[25,5,26,5],[25,6,26,6],[25,7,26,7],[27,0,29,0],[27,1,29,1],[27,4,29,4],[27,5,29,5],[27,6,29,6],[27,7,29,7],[30,0,32,0],[30,1,32,1],[30,4,32,4],[30,5,32,5],[30,6,32,6],[30,7,32,7],[33,0,34,0],[33,1,34,1],[33,4,34,4],[33,5,34,5],[33,6,34,6],[33,7,34,7],[35,0,36,0],[35,1,36,1],[35,4,36,4],[35,5,36,5],[35,6,36,6],[35,7,36,7],[37,0,39,0],[37,1,39,1],[37,4,39,4],[37,5,39,5],[37,6,39,6],[37,7,39,7],[40,0,42,0],[40,1,42,1],[40,4,42,4],[40,5,42,5],[40,6,42,6],[40,7,42,7],[44,0,46,0],[44,1,46,1],[44,4,46,4],[44,5,46,5],[44,6,46,6],[44,7,46,7],[47,0,49,0],[47,1,49,1],[47,4,49,4],[47,5,49,5],[47,6,49,6],[47,7,49,7],[50,0,52,0],[50,1,52,1],[50,4,52,4],[50,5,52,5],[50,6,52,6],[50,7,52,7],[53,0,55,0],[53,1,55,1],[53,4,55,4],[53,5,55,5],[53,6,55,6],[53,7,55,7],[56,0,57,0],[56,1,57,1],[56,4,57,4],[56,5,57,5],[56,6,57,6],[56,7,57,7],[58,0,59,0],[58,1,59,1],[58,4,59,4],[58,5,59,5],[58,6,59,6],[58,7,59,7],[60,0,61,0],[60,1,61,1],[60,4,61,4],[60,5,61,5],[60,6,61,6],[60,7,61,7],[62,0,63,0],[62,1,63,1],[62,4,63,4],[62,5,63,5],[62,6,63,6],[62,7,63,7],[65,0,66,0],[65,1,66,1],[65,4,66,4],[65,5,66,5],[65,6,66,6],[65,7,66,7],[67,0,69,0],[67,1,69,1],[67,4,69,4],[67,5,69,5],[67,6,69,6],[67,7,69,7],[87,0,87,7],[89,0,90,0],[89,1,90,1],[89,5,90,5],[89,6,90,6],[89,7,90,7],[98,0,98,7],[110,0,110,7],[112,0,113,0],[112,1,113,1],[112,5,113,5],[112,6,113,6],[112,7,113,7],[114,0,115,0],[114,1,115,1],[114,5,115,5],[114,6,115,6],[114,7,115,7],[117,0,118,0],[117,1,118,1],[117,5,118,5],[117,6,118,6],[117,7,118,7]],"flags":["formulas_cached_only"]}
["contacts:","Chen ：15818512224",null,"Address:",null,"No. 278, Yongfengsheng Industrial Park, \nGuanhu Street, Longhua District, Shenzhen"]
["Shenzhen Huachuang Micro Vision Technology Co., Ltd. "]
["USB Products"]
["PRODUCT MODEL","Product images","Pixel","Parameters","Cable Length","Size(mm)","Signal type","Interface (optional)"]
["HCU-WJB152\n",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm/90° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-GJ152\n",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : /\nResolution 1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle  2.1mm /120°(optional)\nAudio : Mic\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-CGJ152",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : /\nResolution :1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : Mic\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-WJB282",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 2.8mm /110°(optional)\nAudio : /\nResolution :1280*720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 2.8mm /110°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 2.8mm /110°(optional)\nAudio : Mic\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-XMY152\n",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle  2.36mm /142°(optional)\nAudio : /\nResolution :1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.36mm /142°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle 2.36mm /142°(optional)\nAudio : Mic\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-QJ152",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : /\nResolution :1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : Mic\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : Mic\nResolution :2560X1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-XP152",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : /\nResolution :1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :2560X1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-GJ155",null,"5.0MP","Sensor: 1/4\" COMS\nLens :Wide angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :2560X1440 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"8.0MP","Sensor: 1/3.2\" COMS\nLens :Wide angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :3264X2488 @ 15fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-ZDDJ155(GJ)",null,"5.0MP","Sensor: 1/4\" COMS\nLens :Autofocus wide-angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :2560X1440 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"8.0MP","Sensor: 1/3.2\" COMS\nLens :Autofocus wide-angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :3264X2488 @ 15fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"12.0MP","Sensor: 1/2.5\" COMS\nLens :Autofocus wide-angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :4000x3000  @ 10fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-ZDDJ155",null,"5.0MP","Sensor: 1/4\" COMS\nLens :No distortion 3.57mm /65°(optional)\nAudio : Mic\nResolution :2560X1440 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","15*15","USB"]
[null,null,"8.0MP","Sensor: 1/3.2\" COMS\nLens :No distortion 3.57mm /65°(optional)\nAudio : Mic\nResolution :3264X2488 @ 15fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"12.0MP","Sensor: 1/2.5\" COMS\nLens :No distortion 3.57mm /65°(optional)\nAudio : Mic\nResolution :4000x3000  @ 10fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-GJ155RG",null,"5.0MP","Sensor: 1/4\" COMS\nLens :Wide angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :2560X1440 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","Default 1.5M\nsupports customization","15*15","USB"]
[null,null,"8.0MP","Sensor: 1/3.2\" COMS\nLens :Wide angle 1.9mm /100°(optional)\nAudio : Mic\nResolution :3264X2488 @ 15fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-RG152",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","Default 1.5M\nsupports customization","15*15","USB"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :2560X1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-ZDDJ158RG",null,"5.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.57mm /65°(optional)\nAudio : Mic\nResolution :2560X1440 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","Default 1.5M\nsupports customization","15*15","USB"]
[null,null,"8.0MP","Sensor: 1/3.2\" COMS\nLens :Distortion free 3.57mm /65°(optional)\nAudio : Mic\nResolution :3264X2488 @ 15fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"12.0MP","Sensor: 1/2.5\" COMS\nLens :Distortion free 3.57mm /65°(optional)\nAudio : Mic\nResolution :4000x3000  @ 10fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-JZ192ZK",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.7mm/50° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","19*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.7mm /50°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.7mm /50°(optional)\nAudio :  optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-DBT152",null,"2MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG",null,"15*15","USB"]
["HCU-JZWJB192",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm/90° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","19*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio :optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-JZGJ192",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : /\nResolution 1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","19*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio :optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle  2.1mm /120°(optional)\nAudio :optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-JZQJ192",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : /\nResolution :1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","19*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio :optional\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : optional\nResolution :2560X1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-JZCGJ192",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : /\nResolution :1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","19*15","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio :optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-JZ192RG",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","Default 35CM\nsupports customization","19*15","USB"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :wide angle 1.96mm /150°(optional)\nAudio : optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-BT202(ZFY)",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm/90° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","20*77","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : Mic\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-BTDZ202",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm/90° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","20*77","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-BT182",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.6mm/90° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","18*43","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-BTYS303",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG\nSupport night vision     ","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","30*77","USB"]
["HCU-ZDT202",null,"1.0MP","Sensor: 1/4\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : /\nResolution 1280x720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","20*65","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-ZDT182(ZK)",null,"1.0MP","Sensor: 1/4\" COMS\nLens :Distortion free 3.7mm/50° (optional)\nAudio : /\nResolution:1280X720 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","18*23","USB"]
[null,null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.7mm /50°(optional)\nAudio :optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
[null,null,"4.0MP","Sensor: 1/2.8\" COMS\nLens :Distortion free 3.7mm /50°(optional)\nAudio :optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG"]
["HCU-FK202",null,"2.0MP","Sensor： 1/2.9 \nLens :Manual zoom 2.8-12mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","22*22","USB"]
["HCU-FKWJB202",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","22*22","USB"]
["HCU-FKQJ202",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : optional\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","22*22","USB"]
["HCU-FKGJ252",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.1mm /120°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","25*25","USB"]
["HCU-FK252",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","25*25","USB"]
["HCU-FK302",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","30*30","USB"]
["HCU-FKQJ302",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Panorama 1.5mm /210°(optional)\nAudio : optional\nResolution :1920X1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","30*30","USB"]
["HCU-FKWJB352",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :Distortion free 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","35*35","USB"]
["HCU-FK302B28",null,"2.0MP","Sensor： 1/2.9 \nLens :Manual zoom 2.8-12mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","35*35","USB"]
["HCU-FKGJ362",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 2.8mm /95°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","36*36","USB"]
["HCU-FKMY362",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 2.1mm /170°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","36*36","USB"]
["HCU-FKYS420",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","42*42","USB"]
["HCU-FKCJ252",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 16mm /20°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","25*25","USB"]
["HCU-DMY212",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 2.1mm /170°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","USB"]
["HCU-XMY212",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens :wide angle 2.36mm /142°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG\n","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","USB"]
["HCU-QXCZ552",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG\nSupport night vision     ","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","55*69","USB"]
["HCU-CZ482",null,"2.0MP","Sensor: 1/2.9\" COMS\nLens : 3.6mm /90°(optional)\nAudio : optional\nResolution :1920x1080 @ 30fps\nCable Length:2M (customizable)\nCompressed Format :MJPEG/YUY2\nCompatible system:Android/Windows/Linux\nWorking voltage: DC 5V\nSupport protocol : UVC/OTG\nSupport night vision","(USB2.0) Default  2M\n(Type-C/OTG) Default 1.2M\nsupports small batch customization","48*48","USB"]
["AHD Products"]
["HCA-BT182",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : 3.6mm /90°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V\nAgreement: UTC         ",null,"18*43","AHD","BNC"]
["HCA-C62",null,"1.0MP","Sensor: 1/4\" COMS\nLens : 3.3mm /67°(optional)\nAudio : /\nResolution :1280x720 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V\n",null,"6*6","AHD","BNC"]
[null,null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : 3.3mm /67°(optional)\nAudio : optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V"]
["HCA-C342",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : 3.0mm /60°(optional)\nAudio :support\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V\nSupport night vision     \n      ",null,"10*34","AHD","BNC"]
["HCA-C202",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : 3.6mm /90°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"20*77","AHD","BNC"]
["HCA-CXMY202",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : 2.36mm /142°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"Lens diameter 28\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","AHD","BNC"]
["HCA-WJB152",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : Distortion free 3.6mm /90°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"15*15 ","AHD","BNC"]
["HCA-ZDT182",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : Distortion free 3.6mm /90°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"18*23","AHD","BNC"]
["HCA-ZDT202",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : wide angle 2.1mm /120°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"20*65","AHD","BNC"]
["HCA-C19M",null,"2.0MP","Sensor: 1/2.8\" COMS\nLens : wide angle 2.1mm /120°(optional)\nAudio :optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"19*15","AHD","BNC"]
["CVBS products"]
["HCC-FKQJ202",null,"300000 pixels","Sensor: 1/4\" COMS\nLens :panorama 1.5mm /210°(optional)\nAudio :optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"22*22","CVBS"]
["HCC-FK252",null,"300000 pixels","Sensor: 1/4\" COMS\nLens :wide angle 2.1mm\n /120°(optional)\nAudio :optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"25*25","CVBS"]
["HCC-FK362D",null,"700000 pixels","Sensor：1/3\" CCD           \nLens : 3.7mm /50°(optional)  \nAudio: optional\nResolution :1020x596 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nChip model: NVP2090+811",null,"36*36","CVBS(SNCCD)"]
["HCC-FK302D",null,"700000 pixels","Sensor：1/3\" CCD           \nLens : Distortion free 3.6mm /90°(optional)  \nAudio: optional\nResolution :1020x596 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nChip model: NVP2090+811",null,"30*30","CVBS"]
["HCC-C6",null,"300000 pixels","Sensor：1/6\" COMS             \nLens : Distortion free 3.3mm /60°(optional)\nAudio: optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"6*6","CVBS"]
["HCC-C157",null,"300000 pixels","Sensor：1/4\" COMS             \nLens : Distortion free 3.6mm /90°(optional)\nAudio: optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 3.3V",null,"15*15","CVBS"]
["HCC-NKJ30",null,"300000 pixels","Sensor：1/9\" COMS             \nLens : 3.0mm /60°(optional)\nAudio: optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"5.5*37","CVBS"]
["HCC-C25D",null,"700000 pixels","Sensor：1/3\" CCD            \nLens : 3.6mm /90°(optional)\nAudio: optional\nResolution :1020x596 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nChip model: NVP2090+811",null,"25*25","CVBS"]
["HCC-FK25D02\nWJB",null,"300000 pixels","Sensor：1/3\" CCD            \nLens : 3.6mm /90°(optional)\nAudio: optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nChip model: SONY2463+405AL pure black and white",null,"25*25","CVBS"]
["HCC-ZDT20C",null,"300000 pixels","Sensor：1/4\" COMS             \nLens :wide angle 2.1mm /120°(optional)\nAudio: optional\nResolution :640x480 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\n",null,"20*65","CVBS"]
["HCC-CXMY20D",null,"700000 pixels","Sensor：1/3\" CCD            \nLens :wide angle 2.1mm /170°(optional)\nAudio: optional\nResolution :1020x596 @ 50fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nChip model: NVP2090+811",null,"Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","CVBS"]
["Network products"]
["HCW-FK402WL",null,"2.0MP","Sensor：1/2.9\" COMS           \nLens :wide angle 2.1mm /120°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"40*40","Network","RJ45"]
["HCW-ZDT204WL",null,"2.0MP","Sensor：1/2.9\" COMS           \nLens :wide angle 2.1mm /120°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"20*65","Network","RJ45"]
[null,null,"4.0MP","Sensor：1/2.8\" COMS           \nLens :wide angle 2.1mm /120°(optional)\nAudio: optional\nResolution :2560x1440 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V"]
["HCW-BT204WL",null,"2.0MP","Sensor：1/2.8\" COMS           \nLens : 3.6mm /90°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"20*77","Network","RJ45"]
[null,null,"4.0MP","Sensor：1/2.8\" COMS           \nLens :3.6mm /90°(optional)\nAudio: optional\nResolution :2560x1440 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V"]
["HCW-CZ482",null,"2.0MP","Sensor：1/2.8\" COMS           \nLens : 3.6mm /90°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nSupport night vision",null,"48*48","Network","RJ45"]
["HCW-BTYS204",null,"2.0MP","Sensor：1/2.8\" COMS           \nLens : 3.6mm /90°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V\nSupport night vision",null,"30*77","Network","POE"]
[null,null,"4.0MP","Sensor：1/2.8\" COMS           \nLens :3.6mm /90°(optional)\nAudio: optional\nResolution :2560x1440 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V"]
["HCW-XMY212",null,"2.0MP","Sensor：1/2.8\" COMS           \nLens : wide angle 2.36mm /142°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","Network","RJ45"]
["v380",null,"3.0MP","Sensor：1/2.8\" COMS           \nLens : wide angle 2.1mm /170°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:55CM (customizable)\nWorking voltage: DC 12V",null,"Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","Network","WIFI"]
["HCW-HSMY",null,"3.0MP","Sensor：1/2.9\" COMS           \nLens : wide angle 1.66mm /170°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:2M (customizable)\nWorking voltage: DC 12V\nSupport night vision",null,"Lens diameter 33.5\nMain body diameter 16\nTotal length 89","Network","WIFI"]
["HCW-YSMY",null,"3.0MP","Sensor：1/2.9\" COMS           \nLens : wide angle 1.66mm /170°(optional)\nAudio: optional\nResolution :1920x1080 @ 25fps\nCable Length:2M (customizable)\nWorking voltage: DC 12V\nSupport night vision",null,"Lens diameter 33.5\nMain body diameter 16\nTotal length 89","Network","WIFI"]
["HCW-DMYPOE",null,"4.0MP","Sensor：1/2.9\" COMS           \nLens : wide angle 2.1mm /170°(optional)\nAudio: optional\nResolution :2560x1440 @ 25fps\nCable Length:2M (customizable)\nWorking voltage: DC 12V\n",null,"Lens diameter 31\nMain body diameter 21\nTail cover diameter 35\nTotal length adjustable from 36 to 90","Network","POE"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}